miniDSP USB Audio 2.0 Device Firmware Upgrade steps (For MAC OSX)


1. Copy the miniDSP_UAC2_DFU_OSX into local disk drive

2. Copy and place the firmware (.bin) into the folder

3. Open a terminal

4. change directory to the folder

5. run the below command
	source setup.sh

6. run the below command
	./xmosdfu --download firmware_name.bin

7. The download process should not take more then one minute



miniDSP USB Audio 2.0 Device Firmware Upgrade steps (For Windows)


1. Install the Windows UAC2 Driver

2. Connect the miniDSP UAC2 Device (USBStreamer / miniDSP 2x4n etc....)

3. Run miniDSP UAC2 DFU Tool
	Start Menu -> All Programs -> miniDSP Ltd -> miniDSP USB Audio Class2 Driver -> miniDSP UAC2 DFU Tool

3a. Click "Browse..." and choose file firmware_name.bin

3b. Click "Start" and wait for the progress bar to load, this will take 30 second to a minute

3c. If the stay in "Entering upgrade mode..." for more then 30 second, replug the USB cable



